Golden Lion SAC     Boat safety checklist

	Date
	Site
	Purpose of voyage



	I/c boat for the day
	Dive Marshall


	Boat Launcher
	Person towing


	Diver Cox  

	Passengers/Crew


	Boat handlers

	

	Person carrying out checks

	


All sections to be ticked when complete
Boat equipment 
· Anchor and anchor line and buoy 
· Bucket / bailer, bilge pump 
· Mooring lines and spare ropes 
· Shot line 
· Tubes inflated - bellows 
Engine and Fuel 
· Spare fuel
· 2 stroke oil container full
· Engine spares (spark plugs, shear pins, etc) and tools to fit them 
· Paddles 
· Fuel tank full and pump primed 
· Engine ignition switches operational and 'kill cord' fitted 
· Spare ‘kill cord’ 
Navigation and Safety 
· Voyage Plan(s)
· Compass
· GPS/Sounder
· VHF/DSC Radio 
· Personal buoyancy aids for all who need them (Cox/Crew/passengers)
· Distress flares - Inshore Pack (2 x orange smoke, 2 x red pinpoint or 2 x day / night flares) 
· Fire extinguisher
· First aid kit 
· Oxygen set
· Crew Briefed on locations and use of Emergency Equipment 
Putting away
· Washed down by ________________________
· Engine flushed through
· Any damage/repairs required listed below
· Sheet returned to Boat Officer.

	List here any Essential repairs/ service required before the next voyage




Name of inspector
	

	List here any minor repairs/issues to be aware of on next voyage




Name of inspector
	



Costs
	Amounts spent
	£
	Due to
	Paid

	Fuel
	
	
	

	Launching fees
	
	
	

	Towing
	
	
	

	Other
	
	
	

	
	
	
	



Contributions to use
	Names
	Amounts due
	Paid

	








	
	

	
	
	

	
	
	



Balance to club funds:  £
